

Cables required

Copper cross over cable ------------------

Copper straight Through \_\_\_\_\_\_\_\_\_\_\_\_

Serial DTE / Serial DTC

R1 Commands

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#hostname R1

R1(config)#line console 0

R1(config-line)#password cisco

R1(config-line)#login

R1(config-line)#exit

R1(config)#line vty 0 4

R1(config-line)#password cisco

R1(config-line)#login

R1(config-line)#exit

R1(config)#interface FastEthernet0/0

R1(config-if)#ip address 192.168.1.1 255.255.255.0

R1(config-if)#exit

R1(config)#interface Serial0/0/0

R1(config-if)#ip address 192.168.2.1 255.255.255.0

R1(config-if)#no sh

R1(config-if)#description R2 LAN

R1(config-if)#end

R1#copy running-config startup-config

R1#show running-config

R1# show interfaces fastEthernet 0/0

R1#show version

R1#show ip interface brief

\_\_\_\_\_\_\_\_\_\_\_\_

R2 Commands

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#hostname R2

R2(config)#line console 0

R2(config-line)#password cisco

R2(config-line)#login

R2(config-line)#exit

R2(config)#line vty 0 4

R2(config-line)#password cisco

R2(config-line)#login

R2(config-line)#exit

R2(config)#interface FastEthernet0/0

R2(config-if)#ip address 192.168.3.1 255.255.255.0

R2(config-if)#exit

R2(config)#interface Serial0/0/0

R2(config-if)#ip address 192.168.2.2 255.255.255.0

R2(config-if)#clock rate 64000

R2(config-if)#no sh

R2(config-if)#description R2 LAN

R2(config-if)#end

R2#copy running-config startup-config

R2#show running-config

R2# show interfaces fastEthernet 0/0

R2#show version

R1#show ip interface brief

\_\_\_\_\_\_\_\_\_\_\_\_

**Ping (Verify connection)**

Step 2: Repeat the ping from R1 to PC1.

R1#ping 192.168.1.10

Step 2: Use the tracert command at the Windows command prompt to discover the path that a packet will take from the R1 router to PC1.

C:\>tracert 192.168.1.1

Erasing Router settings


R1#erase startup-config

R1#copy running-config startup-config

Test connection

R1#show ip route

R1#show ip int brief




R

Router>en

Router>config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#



R1- Configuration

Router1(config)#hostname R1

R1(config)#no ip domain-lookup

R1(config)#enable secret class

R1(config)#line console 0

R1(config-line)#password cisco

R1(config-line)#login

R1(config-line)#line vty 0 4

R1(config-line)#password cisco

R1(config-line)#login



R2 – Configuration

Router2(config)#hostname R2

R2(config)#no ip domain-lookup

R2(config)#enable secret class

R2(config)#line console 0


R2(config-line)#password cisco

R2(config-line)#login

R2(config-line)#line vty 0 4

R2(config-line)#password cisco

R2(config-line)#login



R3- configuration

Router3(config)#hostname R3

R3(config)#no ip domain-lookup

R3(config)#enable secret class

R3(config)#line console 0

R3(config-line)#password cisco

R3(config-line)#login

R3(config-line)#line vty 0 4

R3(config-line)#password cisco

R3(config-line)#login

**Task 3- configure interface router**

R1(config-line)#interface fa0/0

R1(config-if)#ip address 172.16.3.1 255.255.255.0

R1(config-if)#no sh

**Configure Serial port**

R1(config-line)#interface s0/0/0

R1(config-if)#ip address 172.16.2.1 255.255.255.0

R1(config-if)#clock rate 64000

R1(config-if)#no sh

***R2 Interface***

R2(config-line)#interface fa0/0

R2(config-if)#ip address 172.16.1.1 255.255.255.0

R2(config-if)#no sh

*Configure serial ports*

R2(config-line)#interface s0/0/0

R2(config-if)#ip address 172.16.2.2 255.255.255.0

R2(config-if)#no sh

R2(config-line)#interface s0/0/1

R2(config-if)#ip address 192.168.1.2 255.255.255.0

R2(config-if)#clock rate 64000

R2(config-if)#no sh

***R3 Interface***

R3(config-line)#interface fa0/0

R3(config-if)#ip address 192.168.2.1 255.255.255.0

R3(config-if)#no sh

R3(config-line)#interface s0/0/0

R3(config-line)#interface s0/0/1

R3(config-if)#ip address 192.168.1.1 255.255.255.0

R2(config-if)#no sh

The subnet mask of PC1 is wrong. In real world, should be 255.255.255.0

Pc 1


**


The subnet mask of PC2 is wrong. In real world, should b 255.255.255.0

Pc2

**

*Pc 3*

**



Static Routing

R1(config)#ip rout 0.0.0.0.0.0.0.0 172.16.2.2

R1 with default route

R2(config)#ip route 192.168.2.0 255.255.255.0 192.168.1.1

R2(config)#ip route 172.16.3.0 255.255.255.0 s0/0/0

R2 with next hub and exit interface

R3(config)#ip route 172.16.0.0 255.255.255.0 192.168.1.2

Now we have to do Static routing

R3

Router(config)#ip route 172.16.1.0 255.255.255.0 s0/0/0

Router(config)#ip route 192.168.1.0 255.255.255.0 s0/0/0

Router(config)#ip route 192.168.2.0 255.255.255.0 s0/0/0

R2

Router(config)#ip route 172.16.3.0 255.255.255.0 s0/0/1

Router(config)#ip route 192.168.2.0 255.255.255.0 s0/0/0

Router(config)#ip route 172.16.1.0 255.255.255.0 s0/0/1

Router(config)#ip route 172.16.2.0 255.255.255.0 s0/0/1

Router(config)#ip route 172.16.3.0 255.255.255.0 s0/0/1

Ping